{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Summary"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Summary","index":0,"n_rows":6,"n_cols":51,"rows_kept":6,"cut":false,"hidden":false,"merged":[]}
[]
[]
["Generation Resource Primary Frequency Response Summary Tool"]
[]
[]
["ID","Time of Frequency Event (UTC)","Generator Operator","Balancing Authority","GADS Generator Unit ID","Planning Case Bus Number","Final PUPFR Performance","Final PUSPFR Performance","Overall Unit Performance","EIA 860 Plant Name (US Only)","EIA 860 Plant Code (US Only)","EIA 860 Generator ID (US Only)","Generator Type","Generator Machine Base (MBASE)(MVA)","Inertia Constant (H)","Droop Setting","Deadband Setting","Maximum Operating Level (Pmax)(HSL)","Minimum Operating Level (Pmin)(LSL)","Grid Nominal Frequency","Data Source","Pre-Event Average Frequency [T(-16) to T(-2)]","Post-Event Average Frequency [T(+20 to T(+52)]","Pre to Post Perturbation Delta Frequency Actual","Post-Event Frequency (t+46)","Pre to Post-Event Delta Frequency Actual (t+46)","High or Low Frequency Event?","Pre-Event Average MW [T(-2 ) to T(-16)]","Post-Event Average MW [T(+20 to T(+52)]","Pre to Post-Event Delta MW Actual","Headroom Available","Footroom Available","Adequate Margin?","Offset (s) Used","Pre-Event Ramp Magnitude","Actual Primary Frequency Response (adjusted)","Expected Primary Frequency Response (Pre)","Expected Primary Frequency Response (Post)","Expected Primary Frequency Response (Ideal)","Expected Primary Frequency Response (Final)","PUPFR Performance","Final PUPFR Performance","Maximum MW Response [T(+46) to T(+60)]","Actual Sustained Primary Frequency Response","Ramp MW Sustained","Actual Sustained Primary Frequency Response (adjusted)","Expected Sustained Primary Frequency Response [T(+46)]","Expected Sustained Primary Frequency Response (Ideal)","Expected Sustained Primary Frequency Response (Final)","PUSPFR Performance","Final PUSPFR Performance"]